CORFE CASTLE PARISH COUNCIL
Permit Holder Parking Facilities

Location: West Street Permit Holder Parking (What3Words/// ///tungsten.libraries.polo)
Date of Assessment: 23rd October 2025	Next Review Date: 23rd October 2026
Assessed by: Michelle Harrington – Proper Officer	Presented To: Full Council (November 2025)
1. Purpose
This assessment identifies and evaluates hazards associated with the use, maintenance, and management of a small gravel car park. The objective is to protect members of the public, staff, and contractors from harm and ensure compliance with health and safety regulations.

2. Description of Asset.
Small 22 space gravel car park for use by permit holders only. 

3. Risk Rating System
	Likelihood
	Description
	Severity
	Description
	Risk Rating

	1
	Rare
	1
	Insignificant (no injury)
	1–4 = Low

	2
	Unlikely
	2
	Minor injury
	5–9 = Medium

	3
	Possible
	3
	Moderate injury
	10–16 = High

	4
	Likely
	4
	Major injury
	17–25 = Critical

	5
	Almost Certain
	5
	Fatality
	


Risk Score = Likelihood × Severity

4. Risk Assessment Table
	Hazard
	Who May Be Harmed
	Initial Risk (L×S)
	Existing Controls
	Further Controls / Actions Required
	Residual Risk

	Uneven surface / loose gravel causing slips, trips, or falls
	Public, staff, contractors
	3×3=9 (Med)
	Fill potholes promptly; Sump added to prevent flooding. 
	
	2×2=4 (Low)

	Vehicle collisions (reversing, poor visibility)
	Drivers, pedestrians
	3×4=12 (High)
	Clear entry/exit area. Users aware to report an issue to Parish Council Clerk. 
	
	2×3=6 (Med)

	Poor lighting at night
	Public, staff
	3×3=9 (Med)
	Existing sensor lighting by toilet block. No further lighting desired to preserve Dark Skies
	
	2×2=4 (Low)

	Weather conditions (ice, snow, flooding)
	Public, staff
	3×4=12 (High)
	Inspect after heavy rainfall
	
	2×3=6 (Med)

	Pedestrian–vehicle interaction
	All site users
	3×4=12 (High)
	Warning signs being added late 2025. 
	
	2×3=6 (Med)

	Potholes or surface erosion
	Public, vehicles
	3×3=9 (Med)
	Regular inspection and maintenance schedule to top up gravel or repair as needed. 
	
	2×2=4 (Low)

	Overhanging vegetation / restricted visibility
	Drivers, pedestrians
	2×2=4 (Low)
	Grounds maintenance schedule & cut back vegetation seasonally
	
	2×2=4 (Low)

	Vandalism or antisocial behaviour (loitering, damage)
	Public, staff
	2×4=8 (Med)
	Community and permit holder involvement
	
	2×3=6 (Med)



5. Emergency Procedures
· Accident or injury: Call emergency services (999) if required; report to Parish Council.
· Fire or vehicle fire: Call emergency services (999), report to Parish Council
· Flooding or ice hazard: Close area temporarily; notify users.
· Vandalism or criminal activity: Do not approach; report to police and afterwards to Parish Council.

6. Personal Protective Equipment (PPE) / Safety
	Task
	PPE Required

	Routine inspection / maintenance
	High-visibility vest, gloves, safety boots for Caretaker or external contractor used with own risk assessment. 

	Traffic control / supervision
	Hi-vis jacket, gloves, two-way radio for Caretaker or external contractor used with own risk assessment



7. Review & Monitoring
· Inspect annually, after severe weather or after layout/usage changes.
· Review after any incident or complaint.

Overall Residual Risk: Low (with all controls in place)
